Description: glass to metal seal, plug-in package, 45 copper cored Alloy 50 leads, #10 CRS housing, with flange, Au finishing on the leads.